All from the Teledyne Impulse Wet-Pluggable Series

* BH-8-FS-S/S (8-pin Circular female bulkhead in stainless steel)
* IL-8-MP (8-pin Circular male with wire)
* DC-8-MP (8-pin Circular male dummy plugs)
* BH-10-FS-S/S (10-pin Circular female bulkhead in stainless steel)
* IL-10-MP (10-pin Circular male with wire)
* DC-10-MP (10-pin Circular male dummy plugs)
* MC-BH-3-FS-S/S , MC-BH-6-FS-S/S, MC-BH-8-FS-S/S, MC-BH-10-FS-S/S, MC-BH-16-FS-S/S (Micro-Mini stainless steel female bulkheads with 3, 6, 8, 10, and 16 pins)
* MC-IL-3-MP, MC-IL-6-MP, MC-IL-8-MP, MC-IL-10-MP, MC-IL-16-MP (Micro-Mini male with wire)
* MC-DC-3-MP, MC-DC-6-MP, MC-DC-8-MP, MC-DC-10-MP, MC-DC-16-MP (Micro-Mini male dummy plugs)
* Do they do male-to-male wires? About 2ft in length.

From the NetG series:

* NETG-FCR (o-ring only)
* NETG-BCR (o-ring + threads)
* NETG-CCR (male)
* NETG-CCP (female)
* Do they do female to female fixed length?